                             Honeywell JavaPOS Driver
                               (c) HONEYWELL, 2012

                            R E L E A S E    N O T E S

Honeywell JavaPOS Driver For Linux 2.03
========================================
1. SUPPORTED Devices
	 ====================================
	|              |        |    USB    |
	| Device       |  RS232 |   Serial  |
	|====================================
	|  1902        |                    |
	|  1900	       |	            |
        |  1200        |   All supported    |
        |  1202        |                    |
	|  1250        |                    |
	|  1300        |                    |
        |  3310g       |                    |
	|  2700	       |                    |
        |-----------------------------------|
	|  2400        |   All supported    | 
        |  9540        |                    |
        |  9520        |                    |  
	 ===================================
	
2. SUPPORTED OSes 
--------------------------------
- CentOS Enterprise 5.7(Kernel 2.6.18)
- Red Hat Linux Enterprise 6.3(Kernel 2.6.32)
- OpenSUSE 11.4(kernel 2.6.37)
- SUSE Linux Enterprise Server 11 SP2 (Kernel 3.0.13)

3. DOCUMENTATION
-----------------
Honeywell JavaPOS Driver For Linux User's Guide.pdf

4. FIXES
--------------
- MTLSO-77 add support for NGB 2700 on¡¡Linux

5. KNOWN ISSUES
----------------
- MTLSO-47: The Validation Utility help file does not exist.
- MTLSO-48: JavaPOS validation utility does not support Configuration Utility.
- MTLSO-56: JavaPOS validation utility does not support any menu command. 
- MTLSO-51: Direct I/O Get BMP image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-52: Direct I/O Get JPEG: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-53: Direct I/O Get Tiff Bin image. Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-54: Direct I/O Get Tiff Grey Image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-58: Update firmware through the select method button is not supported (flashing not supported)
- MTLSO-59: The set PowerNotify does not seem to work (USB Serial Not Supporetd).
- Selection of Device name in JavaPOS Validation Utility throws error message. This is a test Application issue and not a JavaPOS Driver Problem.


6 LIMITATIONS
----------------
- Only USB Serial and RS232 Interfaces are supported.
- Metro USB Serial Interface only works on Linux Kernel 2.6.18, 2.6.27 and 2.6.39
- The following features are not supported: Firmware Flashing, Direct I/O for Menu Commands(Except HHI Scanner - Model Number,Firmware Number,BEEP Command ),and Image Capture
- The following features are not supported: Firmware Flashing, Direct I/O for Menu Commands(Except Legacy Metro Scanner-BEEP Command,U18,Check Health),and Image Capture
- Metro USB Serial Interface does not support methods ¡°CheckHealth¡± and ¡°CheckHealthText¡±.

Honeywell JavaPOS Driver For Linux 2.02
========================================
1. SUPPORTED Devices
	 ====================================
	|              |        |    USB    |
	| Device       |  RS232 |   Serial  |
	|====================================
	|  1902        |                    |
	|  1900	       |	            |
        |  1200        |   All supported    |
        |  1202        |                    |
	|  1250        |                    |
	|  1300        |                    |
        |  3310g       |                    |
        |-----------------------------------|
	|  2400        |   All supported    | 
        |  9540        |                    |
        |  9520        |                    |  
	 ===================================
	
2. SUPPORTED OSes 
--------------------------------
- CentOS Enterprise 5.7(Kernel 2.6.18)
- Red Hat Linux Enterprise 6.3(Kernel 2.6.32)
- OpenSUSE 11.4(kernel 2.6.37)
- SUSE Linux Enterprise Server 11 SP2 (Kernel 3.0.13)

3. DOCUMENTATION
-----------------
Honeywell JavaPOS Driver For Linux User's Guide.pdf

4. FIXES
--------------
- MTLSO-75 EWR09664 linux JPOS Driver is hanging and not providing an execption code when doing very frequent Claim->Enable->Release

5. KNOWN ISSUES
----------------
- MTLSO-47: The Validation Utility help file does not exist.
- MTLSO-48: JavaPOS validation utility does not support Configuration Utility.
- MTLSO-56: JavaPOS validation utility does not support any menu command. 
- MTLSO-51: Direct I/O Get BMP image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-52: Direct I/O Get JPEG: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-53: Direct I/O Get Tiff Bin image. Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-54: Direct I/O Get Tiff Grey Image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-58: Update firmware through the select method button is not supported (flashing not supported)
- MTLSO-59: The set PowerNotify does not seem to work (USB Serial Not Supporetd).
- Selection of Device name in JavaPOS Validation Utility throws error message. This is a test Application issue and not a JavaPOS Driver Problem.


6 LIMITATIONS
----------------
- Only USB Serial and RS232 Interfaces are supported.
- Metro USB Serial Interface only works on Linux Kernel 2.6.18, 2.6.27 and 2.6.39
- The following features are not supported: Firmware Flashing, Direct I/O for Menu Commands(Except HHI Scanner - Model Number,Firmware Number,BEEP Command ),and Image Capture
- The following features are not supported: Firmware Flashing, Direct I/O for Menu Commands(Except Legacy Metro Scanner-BEEP Command,U18,Check Health),and Image Capture
- Metro USB Serial Interface does not support methods ¡°CheckHealth¡± and ¡°CheckHealthText¡±.

Honeywell JavaPOS Driver For Linux 2.01
========================================
1. SUPPORTED Devices
	 ====================================
	|              |        |    USB    |
	| Device       |  RS232 |   Serial  |
	|====================================
	|  1902        |                    |
	|  1900	       |	            |
    	|  1200        |   All supported    |
    	|  1202        |                    |
	|  1250        |                    |
	|  1300        |                    |
        |  3310g       |                    |  
        |-----------------------------------|
	|  2400        |   All supported    | 
        |  9540        |                    |
        |  9520        |                    |  
	 ===================================
	
2. SUPPORTED OSes 
--------------------------------
- CentOS Enterprise 5.7(Kernel 2.6.18)
- Red Hat Linux Enterprise 6.3(Kernel 2.6.32)
- OpenSUSE 11.4(kernel 2.6.37)

3. DOCUMENTATION
-----------------
Honeywell JavaPOS Driver For Linux User's Guide.pdf

4. FIXES
--------------
- MTLSO-69 JPOS SO Crash while claiming an unplugged device

5. KNOWN ISSUES
----------------
- MTLSO-47: The Validation Utility help file does not exist.
- MTLSO-48: JavaPOS validation utility does not support Configuration Utility.
- MTLSO-56: JavaPOS validation utility does not support any menu command. 
- MTLSO-51: Direct I/O Get BMP image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-52: Direct I/O Get JPEG: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-53: Direct I/O Get Tiff Bin image. Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-54: Direct I/O Get Tiff Grey Image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-58: Update firmware through the select method button is not supported (flashing not supported)
- MTLSO-59: The set PowerNotify does not seem to work (USB Serial Not Supporetd).
- Selection of Device name in JavaPOS Validation Utility throws error message. This is a test Application issue and not a JavaPOS Driver Problem.


6 LIMITATIONS
----------------
- Only USB Serial and RS232 Interfaces are supported.
- Metro USB Serial Interface only works on Linux Kernel 2.6.18, 2.6.27 and 2.6.39
- The following features are not supported: Firmware Flashing, Direct I/O for Menu Commands(Except HHI Scanner - Model Number,Firmware Number,BEEP Command ),and Image Capture
- The following features are not supported: Firmware Flashing, Direct I/O for Menu Commands(Except Legacy Metro Scanner-BEEP Command,U18,Check Health),and Image Capture
- Metro USB Serial Interface does not support methods ¡°CheckHealth¡± and ¡°CheckHealthText¡±.

Honeywell JavaPOS Driver 1.7
========================================
1. SUPPORTED Devices
	 ====================================
	|              |        |    USB    |
	| Device       |  RS232 |   Serial  |
	|====================================
	|  1902        |                    |
	|  1900	       |	            |
    	|  1200        |   All supported    |
    	|  1202        |                    |
	|  1250        |                    |
	|  1300        |                    |
	|  2400        |                    | 
        |  9540        |                    |  
	 ===================================
	
2. SUPPORTED OSes 
--------------------------------
- CentOS Enterprise 6.3 Desktop(2.6.32-279.5.2.el6.i686)
- Red Hat Linux Enterprise 5.7 Desktop(2.6.18-274.el5)
- openSUSe 11.4

3. DOCUMENTATION
-----------------
Honeywell JavaPOS Driver User Guide for Linux V1.7

4. FIXES
--------------
- MTLSO-67 JavaPos driver seems to skip a scanned barcode and when you scan the next barcode the skipped one is returned
- MTLSO-68 DeviceDisableClose does not work correctly and causes Metro devices cannot be enabled
- Integrated the driver to support Legacy Metro and Honeywell devices.

5. KNOWN ISSUES
----------------
- MTLSO-47: The Validation Utility help file does not exist.
- MTLSO-48: JavaPOS validation utility does not support Configuration Utility.
- MTLSO-56: JavaPOS validation utility does not support any menu command. 
- MTLSO-51: Direct I/O Get BMP image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-52: Direct I/O Get JPEG: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-53: Direct I/O Get Tiff Bin image. Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-54: Direct I/O Get Tiff Grey Image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-58: Update firmware through the select method button is not supported (flashing not supported)
- MTLSO-59: The set PowerNotify does not seem to work (USB Serial Not Supporetd).
- Selection of Device name in JavaPOS Validation Utility throws error message. This is a test Application issue and not a JavaPOS Driver Problem.


6 LIMITATIONS
----------------
- Only the following scanner interfaces are supported: USB Serial and RS232.
- The following features are not supported: Firmware Flashing, Direct I/O for Menu Commands(Except HHI Scanner - Model Number,Firmware Number,BEEP Command ),and Image Capture
- The following features are not supported: Firmware Flashing, Direct I/O for Menu Commands(Except Legacy Metro Scanner-BEEP Command,U18,Check Health),and Image Capture
- Metro USB Serial Interface only works on Linux Kernel below 2.6.27


Honeywell JavaPOS Driver 1.6
========================================
1. SUPPORTED Devices
	 ====================================
	|              |        |    USB    |
	| Device       |  RS232 |   Serial  |
	|====================================
	|  1902        |                    |
	|  1900	       |	            |
    	|  1200        |   All supported    |
    	|  1202        |                    |
	|  1250        |                    |
	|  1300	       |                    |
	 ===================================
	
2. SUPPORTED OSes 
--------------------------------
- CentOS Enterprise 6.3 Desktop(2.6.32-279.5.2.el6.i686)
- Red Hat Linux Enterprise 5.7 Desktop(2.6.18-274.el5)
- openSUSe 11.4

3. DOCUMENTATION
-----------------
Honeywell JavaPOS Driver User Guide for Linux V1.6

4. FIXES
--------------
- MTLSO-66 Scanner reports error on claim after close procedure 

5. KNOWN ISSUES
----------------
- MTLSO-47: The Validation Utility help file does not exist.
- MTLSO-48: JavaPOS validation utility does not support Configuration Utility.
- MTLSO-56: JavaPOS validation utility does not support any menu command. 
- MTLSO-51: Direct I/O Get BMP image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-52: Direct I/O Get JPEG: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-53: Direct I/O Get Tiff Bin image. Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-54: Direct I/O Get Tiff Grey Image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-58: Update firmware through the select method button is not supported (flashing not supported)
- MTLSO-59: The set PowerNotify does not seem to work (USB Serial Not Supporetd).
- Selection of Device name in JavaPOS Validation Utility throws error message. This is a test Application issue and not a JavaPOS Driver Problem.


6 LIMITATIONS
----------------
- Only the following scanner interfaces are supported: USB Serial and RS232.
- The following features are not supported: Firmware Flashing, Direct I/O for Menu Commands(Except HHI Scanner - Model Number,Firmware Number,BEEP Command ),and Image Capture
- The following features are not supported: Firmware Flashing, Direct I/O for Menu Commands(Except Legacy Metro Scanner-BEEP Command,U18,Check Health),and Image Capture



Honeywell JavaPOS Driver 1.5
========================================
1. SUPPORTED Devices
	 ====================================
	|              |        |    USB    |
	| Device       |  RS232 |   Serial  |
	|====================================
	|  1902        |                    |
	|  1900	       |	            |
    	|  1200        |   All supported    |
    	|  1202        |                    |
	|  1250        |                    |
	|  1300	       |                    |
	|  2400	       |                    | 
	 ===================================
	
2. SUPPORTED OSes 
--------------------------------
- Red Hat Linux Enterprise 5.7 Desktop(2.6.18-274.el5)

3. DOCUMENTATION
-----------------
Honeywell JavaPOS Driver User Guide for Linux V1.5

4. FIXES
--------------
- Integrated the driver to support Legacy Metro and Honeywell devices.

5. KNOWN ISSUES
----------------
- MTLSO-47: The Validation Utility help file does not exist.
- MTLSO-48: JavaPOS validation utility does not support Configuration Utility.
- MTLSO-56: JavaPOS validation utility does not support any menu command. 
- MTLSO-51: Direct I/O Get BMP image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-52: Direct I/O Get JPEG: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-53: Direct I/O Get Tiff Bin image. Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-54: Direct I/O Get Tiff Grey Image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-58: Update firmware through the select method button is not supported (flashing not supported)
- MTLSO-59: The set PowerNotify does not seem to work (USB Serial Not Supporetd).
- Selection of Device name in JavaPOS Validation Utility throws error message. This is a test Application issue and not a JavaPOS Driver Problem.


6 LIMITATIONS
----------------
- Only the following scanner interfaces are supported: USB Serial and RS232.
- The following features are not supported: Firmware Flashing, Direct I/O for Menu Commands(Except HHI Scanner - Model Number,Firmware Number,BEEP Command ),and Image Capture
- The following features are not supported: Firmware Flashing, Direct I/O for Menu Commands(Except Legacy Metro Scanner-BEEP Command,U18,Check Health),and Image Capture


Honeywell JavaPOS Driver 1.4
========================================
1. SUPPORTED Devices
	 ====================================
	|              |        |    USB    |
	| Device       |  RS232 |   Serial  |
	|====================================
	|  1902        |                    |
	|  1900	       |	            |
    	|  1200        |   All supported    |
    	|  1202        |                    |
	|  1250        |                    |
	|  1300	       |                    | 
	 ===================================
	
2. SUPPORTED OSes 
--------------------------------
- openSUSe 11.4

3. DOCUMENTATION
-----------------
Honeywell JavaPOS Driver User Guide for Linux V1.4.3

4. FIXES
--------------
- GS1 DataBar Limited and GS1 DataBar Expanded symbology correctly identified.
- More than one .LCK files will not be crated.

5. KNOWN ISSUES
----------------
- MTLSO-47: The Validation Utility help file does not exist.
- MTLSO-48: JavaPOS validation utility does not support Configuration Utility.
- MTLSO-56: JavaPOS validation utility does not support any menu command. 
- MTLSO-51: Direct I/O Get BMP image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-52: Direct I/O Get JPEG: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-53: Direct I/O Get Tiff Bin image. Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-54: Direct I/O Get Tiff Grey Image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-58: Update firmware through the select method button is not supported (flashing not supported)
- MTLSO-59: The set PowerNotify does not seem to work (USB Serial Not Supporetd).
- Selection of Device name in JavaPOS Validation Utility throws error message. This is a test Application issue and not a JavaPOS Driver Problem.


6 LIMITATIONS
----------------
- Only the following scanner interfaces are supported: USB Serial and RS232.
- The following features are not supported: Firmware Flashing, Direct I/O for Menu Commands, and Image Capture



Honeywell JavaPOS Driver 1.3
========================================
1. SUPPORTED Devices
	 ====================================
	|              |        |    USB    |
	| Device       |  RS232 |   Serial  |
	|====================================
	|  1902        |                    |
	|  1900	       |	            |
    	|  1200        |   All supported    |
    	|  1202        |                    |
	|  1250        |                    |
	|  1300	       |                    | 
	 ===================================
	
2. SUPPORTED OSes 
--------------------------------
- openSUSe 11.4

3. DOCUMENTATION
-----------------
Honeywell JavaPOS Driver User Guide for Linux V1.3

4. FIXES
--------------
- MTLSO-49: Advanced Validation utility can not correctly identify EAN8 symbology.
- Add BEPEXE1 DirectIO Command for BEEP sound.

5. KNOWN ISSUES
----------------
- MTLSO-47: The Validation Utility help file does not exist.
- MTLSO-48: JavaPOS validation utility does not support Configuration Utility.
- MTLSO-56: JavaPOS validation utility does not support any menu command. 
- MTLSO-51: Direct I/O Get BMP image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-52: Direct I/O Get JPEG: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-53: Direct I/O Get Tiff Bin image. Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-54: Direct I/O Get Tiff Grey Image: Image preview box comes up but no image is displayed (Image capture not supported)
- MTLSO-58: Update firmware through the select method button is not supported (flashing not supported)
- MTLSO-59: The set PowerNotify does not seem to work (USB Serial Not Supporetd).
- Selection of Device name in JavaPOS Validation Utility throws error message. This is a test Application issue and not a JavaPOS Driver Problem.


6 LIMITATIONS
----------------
- Only the following scanner interfaces are supported: USB Serial and RS232.
- The following features are not supported: Firmware Flashing, Direct I/O for Menu Commands, and Image Capture

							
							
Honeywell JavaPOS Driver 1.2
========================================
1. SUPPORTED Devices
	 ====================================
	|              |        |    USB    |
	| Device       |  RS232 |   Serial  |
	|====================================
	|  1902        |                    |
	|  1900	       |		    |
        |  1200        |   All supported    |
        |  1202        |                    |
	|  1250        |                    |
	|  1300	       |      		    | 
	 ===================================
	
2. SUPPORTED OSes 
--------------------------------
- openSUSe 11.4

3. DOCUMENTATION
-----------------
Honeywell JavaPOS Driver User Guide for Linux V1.2

4. FIXES
--------------
-MTLSO-43:Data count doesn't get incremented if we use O/C/E
-Change in checkHealth Method (ConnectionDetectRS232 property remove for checkHealth )
-MTLSO-40:Exception message text can be standardized across the Exception windows.
-MTLSO-36:Copy right information mismatch in the application.
-MTLSO-23:Device doesn't scan any barcodes after we perform Open, claim, Release, close operation.
-MTLSO-24:Even the Device name field Empty , the Open method status message shows the device name as "default scanner " failed to open.
-MTLSO-25:Claim Failure doesn't show any status message on the screen.
-MTLSO-33:Clear input properties always throws an execption.
-MTLSO-38:Information displayed on the info window has to be detailed enough.
-MTLSO-39:Irrespective of the Comamnd Retrieve statistics always shows same data.
-Add new feature in JavaPOS Driver Create Logging.

5. KNOWN ISSUES
----------------

6 LIMITATIONS
----------------

==========================================================================================================

Honeywell JavaPOS Driver 1.1
========================================

1. SUPPORTED Devices
	 ====================================
	|              |        |    USB    |
	| Device       |  RS232 |   Serial  |
	|====================================
	|  1902        |                    |
	|  1900	       |		    |
        |  1200        |   All supported    |
        |  1202        |                    |
	|  1250        |                    |
	|  1300	       |                    | 
	 ===================================
	
2. SUPPORTED OSes 
--------------------------------
- openSUSe 11.4

3. DOCUMENTATION
-----------------
- Honeywell JavaPOS Driver User Guide for Linux V1.1

4. FIXES
--------------
- remove dealy in Cliam Method.

5. KNOWN ISSUES
----------------

6 LIMITATIONS
----------------
==========================================================================================================

Honeywell JavaPOS Driver 1.0
========================================

1. SUPPORTED Devices
	 ====================================
	|              |        |    USB    |
	| Device       |  RS232 |   Serial  |
	|====================================
	|  1902        |                    |
	|  1900	       |		    |
        |  1200        |    All supported   |
        |  1202        |                    |
	|  1250        |                    |
	|  1300	       |       		    | 
	 ===================================
	
2. SUPPORTED OSes 
--------------------------------
-  openSUSe 11.4

3. DOCUMENTATION
-----------------
- Honeywell JavaPOS Driver User Guide for Linux V1.0

4. FIXES
--------------
-

5. KNOWN ISSUES
----------------

6 LIMITATIONS
----------------

==========================================================================================================
